
This simple demo uses VisualViewHMI and a Siemens S7-1200.

The HMI shows basic graphic animations. Buttons, gauge, hide/show, move, groups, etc. are used without any scripts.

The RLL program simulates a pump, tank level and several values.

The HMI project is in the “Pump_Tank_Demo_S7-1200_HMI” directory and the RLL project is in the “Pump_Tank_Demo_S7-1200_RLL” directory.

1. The PC needs to be connected to the PLC, with the PLC executing the ladder program.
2. Start PeakHMI and select the project. Select start monitoring. The sample window will open and the elements will be animated.

The simulation window is 1024 * 768.

VisualViewHMI version 4.1.0.8 or higher required.

If you have any problems, questions or comments please contact sales@blftech.com or support@blftech.com

